{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["劳务"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"劳务","index":0,"n_rows":51,"n_cols":10,"rows_kept":51,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,0,1,9],[2,7,2,9],[4,0,4,6],[4,7,4,9],[42,0,42,6],[42,7,42,9],[50,0,50,6],[50,7,50,9],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6]],"flags":["formulas_cached_only"]}
["光明区楼村第四学校项目给水管线迁改工程（劳务分包)报价清单"]
["工程名称:光明区楼村第四学校项目给水管线迁改工程（劳务分包)"]
["序号","项目名称","项目特征描述","计量规则","甲供材","计量\n单位","工程量","金额(元)"]
[{"$nulls":7},"单项控制价","单项投标报价","合价"]
["新建工程",{"$nulls":6},0]
[1,"铸铁管","(1)名称:市政给水管\n(2)规格:球墨铸铁管DN400\n(3)接口方式:橡胶圈柔性接口\n(4)管道检验及试验要求:含管道消毒、冲洗、试压\n(5)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","球墨铸铁管DN400","m",406,70.95,null,0]
[2,"铸铁管","(1)名称:市政给水管\n(2)规格:球墨铸铁管DN150\n(3)接口方式:橡胶圈柔性接口\n(4)管道检验及试验要求:含管道消毒、冲洗、试压\n(5)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","球墨铸铁管DN150","m",20.57,26.45,null,0]
[3,"铸铁管","(1)名称:新建市政中水管\n(2)规格:球墨铸铁管 DN1200\n(3)接口方式:橡胶圈柔性接口\n(4)管道检验及试验要求:含管道消毒、冲洗、试压\n(5)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","球墨铸铁管 DN1200","m",380,140.66,null,0]
[4,"消火栓","(1)名称:地上式室外消火栓\n(2)规格:SS150/65-1.0\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","消火栓","个",3,40.83,null,0]
[5,"挖沟槽土方","(1)名称:挖土方\n(2)土壤类别:综合考虑\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m3",5784.68,7.43,null,0]
[6,"回填方","(1)名称:垫层回填\n(2)填方材料品种:砂砾\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","砂砾","m3",285.73,29.12,null,0]
[7,"回填方","(1)密实度要求:原土回填\n(2)填方材料品种:原土\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m3",3601.13,27.07,null,0]
[8,"场内倒运","(1)名称:场内倒运\n(2)运距:综合考虑，按招标人现场管理要求清理至场内指定位置归堆，由招标人负责外运、投标人配合；\n(3)本项费用包含了场内取土装车、运土等所有工作内容\n(4)工程量计算规则为：投标人综合考虑倒运次数，土方量按图纸一次计算，倒运体积m3=开挖量-回填量-管体体积\n(5)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m3",660.61,58.33,null,0]
[9,"回填方","(1)人工夯填石粉渣,压实\n(2)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m3",1897.81,163.62,null,0]
[10,"室外管道碰头","(1)名称:室外新旧管道连接DN1200\n(2)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"处",2,18692.36,null,0]
[11,"室外管道碰头","(1)名称:室外新旧管道连接DN400\n(2)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"处",5,6467.02,null,0]
[12,"回填液态固化土","1.采用场外加工生产运输。\n2.原料土宜采用开挖弃土，包括砂土、粉土、黏性土等；原料土中块石、混凝土块、砖块等含量不得大于5%，且粒径不得大于10cm。采用泵送方式填筑时，原料土最大粒径不得超过4cm。\n3.固化后28 d 龄期抗压强度为0.3~0.8MPa；\n4.施工前应提供合格的固化土水灰比配合比资料；\n5.回填铸铁管。\n6.采用场外加工生产运输至现场浇筑，包括但不限于生产加工、材料、运输、浇筑等一切费用。","经发包人审核确认的工程量为准","液态固化土","m3",600.67,27.07,null,0]
[13,"混凝土井","(1)名称:地面操作钢砼矩形立式闸阀井\n(2)规格:1400*1800，含井盖井座全套\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","座",2,2916.38,null,0]
[14,"混凝土井","(1)名称:钢筋混凝土矩形排气阀井\n(2)规格:1600*2000，含井盖井座全套\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","座",1,2916.38,null,0]
[15,"混凝土井","(1)名称:钢筋混凝土矩形排气阀井\n(2)规格:1200*1200，含井盖井座全套\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","座",1,2333.1,null,0]
[16,"混凝土井","(1)名称:钢筋混凝土矩形排泥阀井\n(2)规格:1500*2100，含井盖井座全套\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","座",1,2333.1,null,0]
[17,"混凝土井","1.名称:钢筋混凝土矩形排泥阀井\n2.规格:1300*1300，含井盖井座全套\n3.满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","座",1,2333.1,null,0]
[18,"混凝土井","1.名称:钢筋混凝土矩形排泥湿井\n2.规格:Φ1600，含井盖井座全套\n3.满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","座",1,3499.65,null,0]
[19,"混凝土井","1.名称:钢筋混凝土矩形排泥湿井\n2.规格:Φ1000，含井盖井座全套\n3.满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","座",1,1749.83,null,0]
[20,"混凝土支墩","(1)名称:混凝土支墩\n(2)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","m3",420,103.26,null,0]
[21,"现浇构件钢筋","(1)混凝土支墩钢筋\n(2)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","钢筋","t",4.5,1705.35,null,0]
[22,"混凝土包封","(1)名称:混凝土包封\n(2)规格：DN400\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","m",60,84.06,null,0]
[23,"混凝土包封","(1)名称:混凝土包封\n(2)规格：DN1200\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","混凝土","m",62,189.12,null,0]
[24,"钢板桩","(1)名称:钢板桩支护\n(2)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","钢板桩","t",18.3,185.58,null,0]
[25,"标志板","(1)名称:管道标识块\n(2)规格:S30408不锈钢\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","标识牌","块",25,13.4,null,0]
[26,"警示(示踪)带铺设","(1)名称:警示带\n(2)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m",786,2.77,null,0]
[27,"钢管管件制作、安装","(1)名称:11.25°-90°弯头\n(2)规格:DN1200\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","弯头","个",12,296.27,null,0]
[28,"钢管管件制作、安装","(1)名称:11.25°-90°弯头\n(2)规格:DN400\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","弯头","个",15,1332.77,null,0]
[29,"钢管管件制作、安装","(1)名称:排泥三通\n(2)规格:DN1200*600\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","排泥三通","个",1,1927.5,null,0]
[30,"钢管管件制作、安装","(1)名称:排泥三通\n(2)规格:DN400*200\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","排泥三通","个",1,1174.96,null,0]
[31,"钢管管件制作、安装","(1)名称:排气三通\n(2)规格:DN1200*150\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","排气三通","个",1,2144.37,null,0]
[32,"钢管管件制作、安装","(1)名称:排气三通\n(2)规格:DN400*80\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","排气三通","个",1,905.02,null,0]
[33,"阀门","(1)名称:软密封闸阀\n(2)规格:DN400，配双边伸缩器\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","DN400闸阀（配双边伸缩器）","个",2,408.29,null,0]
[34,"阀门","(1)名称:排气阀\n(2)规格:DN150，配双边伸缩器\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","DN150排气阀（配双边伸缩器）","个",1,174.98,null,0]
[35,"阀门","(1)名称:排气阀\n(2)规格:DN80，配双边伸缩器\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","DN80排气阀（配双边伸缩器）","个",1,116.66,null,0]
[36,"阀门","(1)名称:排泥阀，硬密封闸阀\n(2)规格:DN600，配双边伸缩器\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","DN600排泥阀（配双边伸缩器）","个",1,583.28,null,0]
[37,"阀门","(1)名称:排泥阀，硬密封闸阀\n(2)规格:DN200，配双边伸缩器\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准","DN200排泥阀（配双边伸缩器）","个",1,233.31,null,0]
["拆除工程",{"$nulls":6},0]
[38,"拆除铸铁管","(1)名称:拆现状管\n(2)规格:DN300\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m",368.8,55.96,null,0]
[39,"拆除铸铁管","(1)名称:拆现状管\n(2)规格:DN1200\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m",208,131.09,null,0]
[40,"拆除水泥混凝土","(1)名称:拆除现状路面\n(2)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m2",767.22,17.15,null,0]
[41,"挖沟槽土方","(1)名称:挖土方\n(2)土壤类别:综合考虑\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m3",2232.71,8.18,null,0]
[42,"回填方","(1)密实度要求:原土回填\n(2)填方材料品种:原土\n(3)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m3",2512.7,29.76,null,0]
[43,"场内倒运","(1)名称:场内倒运\n(2)运距:综合考虑，按招标人现场管理要求清理至场内指定位置归堆，由招标人负责外运、投标人配合；\n(3)本项费用包含了场内取土装车、运土等所有工作内容\n(4)工程量计算规则为：投标人综合考虑倒运次数，土方量按图纸一次计算，倒运体积m3=开挖量-回填量-管体体积\n(5)满足设计图纸、相关规范、招标文件及其技术要求","经发包人审核确认的工程量为准",null,"m3",280,64.17,null,0]
[44,"拆除室外消火栓","(1)名称:地上式室外消火栓拆除\n(2)规格:SS150/65-1.0","经发包人审核确认的工程量为准",null,"套",2,39.41,null,0]
["合    计",{"$nulls":6},0]